**Transmitter Buoy**

Power on with switch.

Red LED on GPS module will blink until it has a fix.

When it gets a fix, display will show fix.

As soon as it has fix, it will try to send GPS via Iridium

After sending, it will go to sleep for 10 minutes, and then restart the process.

When sleeping, display will show message that was sent.

**Receiver**

Power on with switch.

UP and DN scroll through messages

EN used to check for new messages. This costs about $0.10 a check.